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	STORAGE TANK CONSTRUCTION OPERATIVE
NAECI Grade 5 — Plater 



	Key Function
To assist in the site erection, assembly and construction of large above-ground storage tanks in accordance with applicable standards, drawings, procedures and quality requirements.
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	Main Duties & Responsibilities

	1. To ascertain job requirements from drawings or other specifications.
1. To mark out and develop profiles on plate, structural steelwork, tanks and pipework.
1. To produce templates for marking and/or drilling.
1. To set out plate work for structural steelwork fabrication and Tank Erection.
1. To produce and install structural steelwork fabrications.
1. To produce and install plate work assemblies of square, rectangular, cylindrical or conical form.
1. To produce and install heavy steelwork beams or sections.
1. To produce and install structural lattice girders.
1. To use manual metal arc welding to tack weld fabrications or structural steelwork.
1. To use straight line and profile cutting for any apertures in the Tank Shell, Roof or Floor. 
1. To adhere to all safety requirements including safety checks of tools and equipment.
1. To use Oxy/fuel hand burning/heating/cutting equipment.
1. To use all relevant workshops/site equipment associated with job requirements including all relevant training/certification requirements.
1. To undertake any additional tasks reasonably requested by the Charge-hand, Supervisor or Project Manager consistent with the operative's competence and NAECI Grade 5 classification.



	Qualifications and Experience

	Mandatory Qualifications
1. Approved Apprenticeship to City & Guilds NVQ level 3.
1. Valid Site Safety Passport — CCNSG Safety Passport or equivalent (e.g. CSCS, CISRS) accepted.
Desirable Qualifications & Experience
1. Previous plating experience on above-ground storage tank construction or heavy industrial site fabrication.
1. Familiarity with tank construction standards such as BS EN 14015 or API 650.
1. Confined Space Entry – Medium Risk Training




	NAECI Classification & Pay Framework

	This role is classified as a Grade 5 — Plater under the National Agreement for the Engineering Construction Industry (NAECI). The operative shall be remunerated in accordance with the current NAECI Basic Rates of Pay, Supplementary Payments and Project Agreement (where applicable). Hours, overtime, travel, lodging allowances and welfare provisions shall be as specified in the relevant NAECI schedules and any site-specific Project Agreement in force.



	Health, Safety & Environment

	1. The operative shall at all times comply with the requirements of the Health & Safety at Work etc. Act 1974, the Management of Health & Safety at Work Regulations 1999, and all applicable site-specific Health, Safety & Environment rules and procedures.
1. The operative shall cooperate with the Company's efforts to fulfil statutory obligations and shall not endanger themselves or others through their acts or omissions.
1. Any unsafe acts, conditions or incidents shall be reported to the Supervisor immediately.
1. The operative shall make proper use of all PPE and safety equipment provided, and shall participate in all mandatory safety briefings, toolbox talks and inductions.



	Conclusion

	1. This job profile sets out the main duties and responsibilities of the job holder. It does not constitute an exhaustive or comprehensive description of duties and the job holder will be required to carry out any additional tasks as and when requested to do so by their manager.
1. Responsibilities and duties may also change in light of future business needs and personal development.
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